YES NO YES NO

Do Nothing

Open The Servo Motors, Set flag = 0

Close The Servo Motors, Set flag = 1

Flag = 1?

EMG envelope> EMG Threshold

Process the EMG signal in Arduino Nano

Process the EMG signal in Muscle BioAmp Candy

Get the EMG signal from forearm

Start